{"text_format":"1","workbook":"xlsx","n_sheets":6,"sheets":["VM-AA-310","Homework Survey","Projects","Manufacturers","Items","MiscValues"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"VM-AA-310","index":0,"n_rows":26,"n_cols":5,"rows_kept":26,"cut":false,"hidden":false,"merged":[[3,2,3,4]]}
["Carolina C. Lyon Interior Design"]
["1052 Canyon Meadow Drive Apt 3, Provo UT, 84606 (714) 345-2334"]
[]
["FF&E","Art and Accessories","Item Number: VM-AA-310"]
["Project Name:","Vista Manor Nursing & Rehab",null,"Date:","2012-04-09"]
["Project Location:","San Jose, CA",null,"Reveised Date:"]
["Manufacturer Source:",null,"Product Image:"]
["RBF Group International"]
["1441 W. 2nd St"]
["Pomona CA, 91766"]
["Phone:  (626) 333-5700"]
["Email/WebSite:  http://rbfgroup.net/"]
[]
[]
[]
["Vendor Representative:"]
["RBF Group International"]
["Sarah Sherman"]
["Phone:  (310) 403-7786"]
["Email/Web: sshermansales@gmail.com"]
[]
[]
[]
[]
[]
["Product Information:",null,"Notes:"]

{"sheet":"Homework Survey","index":1,"n_rows":19,"n_cols":17,"rows_kept":19,"cut":false,"hidden":true,"merged":[[19,2,19,16]]}
[]
[]
[]
[]
[null,"Homework Assignment Survey",null,null,null,null,null,null,null,null," Very Strongly Disagree"," Strongly Disagree"," Disagree"," Neither Agree nor Disagree"," Agree"," Strongly Agree"," Very Strongly Agree"]
[null,null,"I feel that this homework was valuable to my learning in the course."]
[]
[null,null,"I enjoyed completing this asignment."]
[]
[null,null,"I feel that it was fair for the professor to expect students to "]
[null,null,"complete this assignment given what we've learned in class so far."]
[]
[null,null,"I feel that this  this assignment was too easy to be meaningful."]
[]
[null,null,"I feel that this assignment was too hard to be meaningful."]
[]
[null,null,"Completing this assignment, I spent appoximately:",null,null,null,null,null,null,null,null," hours   and ",null,null,null," minutes"]
[]
[null,null,"Comments to the professor regarding this assignment:"]

{"sheet":"Projects","index":2,"n_rows":8,"n_cols":4,"rows_kept":8,"cut":false,"hidden":false,"merged":[]}
["ProjectID","ProjectName","ProjectLocation","Abreviation"]
[1001,"Vista Manor Nursing & Rehab","San Jose, CA","VM"]
[1002,"Plum Tree Nursing & Rehab","Los Gatos, CA","PT"]
[1003,"Friendship Manor Nursing & Rehab","National City, CA","FM"]
[1004,"Olds' Residence","Irvine, CA","OR"]
[1005,"Arbor Hills Nursing & Rehab","La Mesa, CA","AH"]
[1006,"Cedar Crest Nursing & Rehab","Sunnyvalle, CA","CC"]
[1007,"Newport Nursing & Rehab","Newport Beach, CA","NP"]

{"sheet":"Manufacturers","index":3,"n_rows":6,"n_cols":13,"rows_kept":6,"cut":false,"hidden":false,"merged":[]}
["Manufac ID","Manfac Name","Address","City","State","Zip","Phone","Email","Vendor Name","Rep Name","Rep Phone","Rep Email","Fax"]
[2001,"RBF Group International","1441 W. 2nd St","Pomona","CA",91766,"(626) 333-5700","http://rbfgroup.net/","RBF Group International","Sarah Sherman","(310) 403-7786","sshermansales@gmail.com","(626) 333-5744"]
[2002,"Hunter Douglas","2211 N Elston Avenue, Ste 301","Chicago","IL",60614,"(800) 229-5300","hunterdouglas.com","SK Associeate","Sarah Krauser","(949) 351-1355","skrauserdesign@cox.net","(773) 634-5123"]
[2003,"Fabricut Contract","9303 East 46th Street","Tulsa","OK",74145,"(800) 999-5533","http://www.fabricutcontract.com/","Fabricut Contract","Mindy Shannon","(818) 635-7937","mindy.shannon@fabricut.com","(918) 665-1117"]
[2004,"Visual Comfort","2021 Bingle Road","Houston","TX",77055,"(713) 686-5999","http://www.visualcomfort.com/","Circa Lighting","Kristi Olson","(912) 442-1008","kristi@circalighting.com"]
[2005,"Good Fellas Industries","1849 East 50th Street","Los Angeles","CA",90058,"(323) 233-2500",null,"Good Fellas Industries","Maggie Reitz","(714) 713-3313","m.reitz.gfi@gmail.com","(323) 233-2539"]

{"sheet":"Items","index":4,"n_rows":8,"n_cols":5,"rows_kept":8,"cut":false,"hidden":false,"merged":[]}
["Spec Type","Item","Item Code","Product Information","Notes"]
["FF&E","Area Rug","IF","Description:\nLocation:\nDesign Pattern:\nQuality:\nContent:\nColor: \nEdge:\nType:\nWidth:\nMaterial:\nColor:\nDimensions: \nSize:\nTotal thickness:\nPattern Repeat: \nInstallation: \nMethod: \nUnderlayment Pad (provide no-skid underlayment pad) \nPerformance Testing: \nFlame Spread: \nSmoke Development.\nDescription:\nLocation:\nDesign Pattern:\nQuality:\nContent:\nColor: \nEdge:\nType:\nWidth:\nMaterial:\nColor:\nDimensions: \nSize:\nTotal thickness:\nPattern Repeat: \nInstallation: \nMethod: \nUnderlayment Pad (provide no-skid underlayment pad) \nPerformance Testing: \nFlame Spread: \nSmoke Development.\n","Field verify all dimensions prior to fabrication\n\nAll products, materials, construction, & installation used must be suitable to use in tropical and high humidity environments.\n\nAll products, materials, construction, & installation used must meet contract quality standards.\n\nAll products, materials, construction, & installation used must meet all local, state, and federal accessibility codes.\n\nAll products, materials, construction, & installation used must meet all local state and federal fire and life safety codes.\n\nSubmittals: Submit a minimum of 2 samples of rug and underlayment to Interior Designer for approval prior to purchase and production.\n"]
["FF&E","Art and Accessories","AA","Description:\n\nLocation:\n\nDimensions:\nImage Dimensions:\nCropping Instructions:\nOutside Dimensions:\nGlazing: \nType: \nMat:\nName:\nColor: \nSize:\nFrame:\nHardware: Security Hardware\n","Insure that item will fit in all elevators, through doors, and corridors prior to commencing fabrication.\n\nAll wood products are to be treated to be insect and vermin free\n\nAll products, materials, construction, & installation used must meet contract quality standards.\n\nAll products, materials, construction, & installation used must meet all local, state, and federal accessibility codes.\n\nAll products, materials, construction, & installation used must meet all local state and federal fire and life safety codes.\n\nSubmittals: Submit a minimum of 2 frame profile samples to Interior Designer for approval prior to purchase and production.\n\n"]
["FF&E","Bedding","IF","Description:\n\nType:\nDesign:\nStyle: \nQuilt Pattern: \nCorner: \nEdge:\nWelt:\nPillow Tuck:\nConstruction:\nCorners: All corners to be mitered\nClosure:\nThread: All thread to be monofilament or triple strand washable polyester in color to match fabric\nSeams: Pattern Match\nQuilting: Continuous quilting with equal lock stitches at 8-10 stitches per inch \nHems: Double blind-stitch hem\nInsert:\nType:\nInsert:\nFill Weight:\nInsert Lining:\nInsert Attachment:\nDimensions:\nBed Size:\nLength:\nWidth:\nDrop:\nDimension Above Finished Floor:\nFace Fabric:\nFabric:\nFabric Direction:\nFabric Width:\nWelt Material: \nSize:\nLocation:\nLining:\nFabric:\nCleaning Method: Machine washable.\nDescription:\n\nType:\nDesign:\nStyle: \nQuilt Pattern: \nCorner: \nEdge:\nWelt:\nPillow Tuck:\nConstruction:\nCorners: All corners to be mitered\nClosure:\nThread: All thread to be monofilament or triple strand washable polyester in color to match fabric\nSeams: Pattern Match\nQuilting: Continuous quilting with equal lock stitches at 8-10 stitches per inch \nHems: Double blind-stitch hem\nInsert:\nType:\nInsert:\nFill Weight:\nInsert Lining:\nInsert Attachment:\nDimensions:\nBed Size:\nLength:\nWidth:\nDrop:\nDimension Above Finished Floor:\nFace Fabric:\nFabric:\nFabric Direction:\nFabric Width:\nWelt Material: \nSize:\nLocation:\nLining:\nFabric:\nCleaning Method: Machine washable.\n\n\nType:\nDesign:\nStyle: \nQuilt Pattern: \nCorner: \nEdge:\nWelt:\nPillow Tuck:\nConstruction:\nCorners: All corners to be mitered\nClosure:\nThread: All thread to be monofilament or triple strand washable polyester in color to match fabric\nSeams: Pattern Match\nQuilting: Continuous quilting with equal lock stitches at 8-10 stitches per inch \nHems: Double blind-stitch hem\nInsert:\nType:\nInsert:\nFill Weight:\nInsert Lining:\nInsert Attachment:\nDimensions:\nBed Size:\nLength:\nWidth:\nDrop:\nDimension Above Finished Floor:\nFace Fabric:\nFabric:\nFabric Direction:\nFabric Width:\nWelt Material: \nSize:\nLocation:\nLining:\nFabric:\nCleaning Method: Machine washable.\nDescription:\n\nType:\nDesign:\nStyle: \nQuilt Pattern: \nCorner: \nEdge:\nWelt:\nPillow Tuck:\nConstruction:\nCorners: All corners to be mitered\nClosure:\nThread: All thread to be monofilament or triple strand washable polyester in color to match fabric\nSeams: Pattern Match\nQuilting: Continuous quilting with equal lock stitches at 8-10 stitches per inch \nHems: Double blind-stitch hem\nInsert:\nType:\nInsert:\nFill Weight:\nInsert Lining:\nInsert Attachment:\nDimensions:\nBed Size:\nLength:\nWidth:\nDrop:\nDimension Above Finished Floor:\nFace Fabric:\nFabric:\nFabric Direction:\nFabric Width:\nWelt Material: \nSize:\nLocation:\nLining:\nFabric:\nCleaning Method: Machine washable.\nDescription:\n\nType:\nDesign:\nStyle: \nQuilt Pattern: \nCorner: \nEdge:\nWelt:\nPillow Tuck:\nConstruction:\nCorners: All corners to be mitered\nClosure:\nThread: All thread to be monofilament or triple strand washable polyester in color to match fabric\nSeams: Pattern Match\nQuilting: Continuous quilting with equal lock stitches at 8-10 stitches per inch \nHems: Double blind-stitch hem\nInsert:\nType:\nInsert:\nFill Weight:\nInsert Lining:\nInsert Attachment:\nDimensions:\nBed Size:\nLength:\nWidth:\nDrop:\nDimension Above Finished Floor:\nFace Fabric:\nFabric:\nFabric Direction:\nFabric Width:\nWelt Material: \nSize:\nLocation:\nLining:\nFabric:\nCleaning Method: Machine washable.\nDescription:\n\nType:\nDesign:\nStyle: \nQuilt Pattern: \nCorner: \nEdge:\nWelt:\nPillow Tuck:\nConstruction:\nCorners: All corners to be mitered\nClosure:\nThread: All thread to be monofilament or triple strand washable polyester in color to match fabric\nSeams: Pattern Match\nQuilting: Continuous quilting with equal lock stitches at 8-10 stitches per inch \nHems: Double blind-stitch hem\nInsert:\nType:\nInsert:\nFill Weight:\nInsert Lining:\nInsert Attachment:\nDimensions:\nBed Size:\nLength:\nWidth:\nDrop:\nDimension Above Finished Floor:\nFace Fabric:\nFabric:\nFabric Direction:\nFabric Width:\nWelt Material: \nSize:\nLocation:\nLining:\nFabric:\nCleaning Method: Machine washable.\n\n\nType:\nDesign:\nStyle: \nQuilt Pattern: \nCorner: \nEdge:\nWelt:\nPillow Tuck:\nConstruction:\nCorners: All corners to be mitered\nClosure:\nThread: All thread to be monofilament or triple strand washable polyester in color to match fabric\nSeams: Pattern Match\nQuilting: Continuous quilting with equal lock stitches at 8-10 stitches per inch \nHems: Double blind-stitch hem\nInsert:\nType:\nInsert:\nFill Weight:\nInsert Lining:\nInsert Attachment:\nDimensions:\nBed Size:\nLength:\nWidth:\nDrop:\nDimension Above Finished Floor:\nFace Fabric:\nFabric:\nFabric Direction:\nFabric Width:\nWelt Material: \nSize:\nLocation:\nLining:\nFabric:\nCleaning Method: Machine washable.\n","Fabricator to verify all yardage requirements\n\nAll products, materials, construction, & installation used must be suitable to use in tropical and high humidity environments.\n\nAll products, materials, construction, & installation used must meet contract quality standards.\n\nAll products, materials, construction, & installation used must meet all local, state, and federal accessibility codes.\n\nSubmittals: Submit one mock-up sample to Interior Designer for approval prior to purchase and production.\n"]
["FF&E","Casegoods","IF","Description:\nLocation:\nDimensions:\nWidth:\nDepth:\nHeight:\nFinish:\nQuantity:\nGlides and Casters: Nylon Glides for Carpet\n","Insure that item will fit in all elevators, through doors, and corridors prior to commencing fabrication.\n\nAll wood products are to be treated to be insect and vermin free\n\nAll products, materials, construction, & installation used must meet contract quality standards.\n\nAll products, materials, construction, & installation used must meet all local, state, and federal accessibility codes.\n\nAll products, materials, construction, & installation used must meet all local state and federal fire and life safety codes.\n\nSubmittals: Submit a minimum of 2 finish samples to Interior Designer for approval prior to purchase and production.\n"]
["FF&E","Fabric","F","Description:\nName:\nNumber:\nColor:\nWidth:\nRepeat:\nAbrasion:\nContent:\nFinish:\nFlammability:\nCleaning:\nQuantity:\n","Manufacturer to provide CLID 1 cutting for approval for designer approval prior to shipping to address noted above"]
["FF&E","Hardware","HW"]
["FF&E","Window Treatment","WT"]

{"sheet":"MiscValues","index":5,"n_rows":4,"n_cols":2,"rows_kept":4,"cut":false,"hidden":false,"merged":[]}
["SpecType","Next Spec Number"]
["FF&E",311]
["GC"]
["Other"]